**A: St Senan’s Church, Clonlara, Co Clare**

Erected in 1870, St Senan’s Church is built of limestone in the early English style and was designed by W.E. Corbett, Limerick. The mainentrance has a large deep recessed molded cut stone door case over which is a cut stone, three light window. The sacristy at the rear is an elaborate structure with cut stone dressings to the windows.

The nave of the Church is 84 feet long and 35 feet wide and the chancel is 24 x 20 ft. It is divided from the nave by a cut stone arch. The height of the nave from the floor to the ridge of the roof is 50ft.

The interior roof of the nave is of open construction and is supported by neatly designed, stained and polished, pine principals and rafters.

The nave is litfrom the sides by eight lancet windows of plain quarry glass set in a diamond pattern with a red glass border.

Ref: Church of St Senan Clonlara, Fr Michael Lane, Shravokee, Clonlara, Co